Performance of C = αAB + βC on 64 processor configurations of the Intel Paragon with GP nodes, the Cray T3D, and the IBM SP-2. The blocking sizes on the Paragon are nb_{alg} = nb = 20 and on the T3D and SP-2 are nb_{alg} = nb = 64.